//Firstly,Every LCD_IO Pins can't be connected with Arduino Pins directly,Every IO Pins should Connecte with a 200¦¸~2K¦¸ Resistor In series.
//As shown in the figure below:
//                     ______________________
//----LCD IO pins-----|_200¦¸~2K¦¸ Resistor__|-----Arduino UNO IO Pins---------
//
/***********************************************************
//IO connection instructions:
//LCD_Model Pin_SDA/SDI/MOSI Connect to Arduino_UNO Pin11
//LCD_Model Pin_SCL/CLK/SCLK Connect to Arduino_UNO Pin10
//LCD_Model Pin_CS/CE Connect to Arduino_UNO Pin9
//LCD_Model Pin_RST/RESET Connect to Arduino_UNO Pin12
//LCD_Model Pin_RS/DC Connect to Arduino_UNO Pin8
/**********************************************************
//Power connection instructions:
//VCC:Connect to 5V DC.
//GND:Connect to Ground.
//BL: Connect to High Level(or VCC),Backlight ON;
//    Low Level(or GND) Backlight OFF.
/**********************************************************
//Note:The "UTFT.zip" library should be Install firstly,if not so, the program won't be correctly compile.
/**********************************************************

